
	Category
	Slow AC recharging point
	Medium-speed recharging point AC recharging point, triple-phase
	Fast AC recharging point, triple-phase
	Slow DC recharging point
	Fast DC recharging point
	Level 1 - Ultra-fast DC recharging point
	Level 2 - Ultra-fast DC recharging point
	Overall total number of points, as of end-May 2026

	(maximum power output)
	(P < 7,4 kW)
	(7,4 kW ≤ P ≤ 22 kW)
	(P > 22 kW)
	(P < 50 kW)
	(50 kW ≤ P < 150 kW)
	(150 kW ≤ P < 350 kW)
	(P ≥ 350 kW)
	

	per AFIR Annex III classification.
	 
	 
	 
	 
	 
	 
	 
	

	Number of Points per Category (as of end May)
	25
	117
	63
	10
	44
	59
	-
	318



